
4.3	Describe how to access and use Safety Data Sheets (SDS) for the safe use, handling and disposal of a hazardous product.

The safety data Sheets (SDS) must be easily available to all workers in the workplace at all times. The SDS may be stored in paper form in a binder or electronically on a computer system.
Training on where to find the SDS, how to access and interpret them is required for all workers.
Prior to using the hazardous product, the worker should review the SDS, in its entirety, for important safe use, handing and disposal information.
The following are some examples of where to find some of the information needed for the safe use, handling and disposal of a hazardous product (e.g. liquid nitrogen).
Section 2 – Hazards identification quickly identifies the hazard by displaying the hazard pictogram and grouping it with the signal word and hazard statement as highlighted by arrows on Figure 6.
Precautionary statements also provide a quick reference in this section.


Figure 6: Safety Data Sheet (SDS) - Section 2 – Hazards Identification




Section 7 – Handling and Storage provides information on how to safety handle and store the hazardous product. The example in Figure 7 gives instructions for protective measures, occupational hygiene and conditions for safe storage. It refers the worker to Section 8 for information on appropriate personal protective equipment.


Figure 7: Safety Data Sheet (SDS) - Section 7 – Handling and Storage


Section 8: Exposure controls/personal protection informs the worker of what, if any, personal protective equipment needs to be worn to protect the worker from the hazard. In Figure 8 it is recommended that chemical resistant, impervious gloves be worn at all times and that the gloves must be insulated and suitable for low temperatures. Safe eyewear should also be worn if there is a possibility of exposure to liquid splashes, mist, gases or dust.




Figure 8: Safety Data Sheet (SDS) - Section 8 – Exposure Controls/Personal Protection


Section 13 – Disposal considerations provides the worker with information of how to safely dispose of waste, recyclable and non-recyclable products. Figure 9 show that waste should be disposed of safety, complying with the environmental protection and waste disposal legislation of the local authority.




Figure 9: Safety Data Sheet (SDS) - Section 13 – Disposal considerations
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+ Personal protective equipment for the body should be selected based on the task being

performed and the risks involved and should be approved by a specialist before
handling this product

: Appropriate footwear and any additional skin protection measures should be selected

based on the task being performed and the risks involved and should be approved by a
specialist before handling this product

+ Use a properly fitted, air-purifying or air-fed respirator complying with an approved

standard if a risk assessment indicates this is necessary. Respirator selection must be
based on known or anticipated exposure levels, the hazards of the product and the safe
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Section 13. Disposal considerations

Disposal methods + The generation of waste should be avoided or minimized wherever possible. Disposal
of this product, solutions and any by-products should at all times comply with the
requirements of environmental protection and waste disposal legislation and any
regional local authority requirements. Dispose of surplus and non-recyclable products
via a licensed waste disposal contractor. Waste should not be disposed of untreated to
the sewer unless fully compliant with the requirements of all authorities with jurisdiction.
Empty Airgas-owned pressure vessels should be retumed to Airgas. Waste packaging
should be recycled. Incineration or landfill should only be considered when recycling is
not feasible. This material and its container must be disposed of in a safe way. Empty
containers or liners may retain some product residues. Do not puncture or incinerate
container
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Section 2. Hazards identification

OSHAJHCS status : This material is considered hazardous by the OSHA Hazard Communication Standard
(29 CFR 1910.1200).
Classification of the : GASES UNDER PRESSURE - Refrigerated liquefied gas

substance or mixture

GHS Iabel elements
Hazard pictograms

Signal word : Waming

Hazard statements + Contains refrigerated gas; may cause cryogenic bums or injury.
May cause frostbite.

: Read and follow all Safety Data Sheets (SDS'S) before use. Read label before use.
Keep out of reach of children. If medical advice is needed, have product container or
label at hand. Close valve after each use and when empty. Use equipment rated for
cylinder pressure. Do not open valve until connected to equipment prepared for use.
Use a back flow preventative device in the piping. Use only equipment of compatible
materials of construction. Always keep container in upright position. Do not change or
force fit connections. Avoid spills. Do not walk o roll equipment over spills.

Prevention : Wear cold insulating gloves and face shield
Use and store only outdoors or in a well ventilated place.
Response : Thaw frosted parts with lukewarm water. Do not rub affected area. Getimmediate
medical attention.
Storage : Store in a well-ventiated place.
Disposal + Not applicable
Hazards not otherwise + Liquid can cause bums similar to frostbite.
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Section 7. Handling and storage

Precautions for safe handling

Protective measures : Puton appropriate personal protective equipment (see Section 8). Contains gas under
pressure. Contains refrigerated gas. Do not get in eyes or on skin or clothing. Avoid
breathing gas. Empty containers retain product residue and can be hazardous. Do not
puncture or incinerate container. Use equipment rated for cylinder pressure. Close
valve after each use and when empty. Protect cylinders from physical damage; do not
drag, roll, side, or drop. Use a suitable hand truck for cylinder movement.

Never allow any unprotected part of the body to touch uninsulated pipes or vessels that
contain cryogenic liquids. Prevent entrapment of liquid in closed systems or piping
without pressure relief devices. Some materials may become brite at low temperatures
and will easily fracture.

Advice on general + Eating, drinking and smoking should be prohibited in areas where this materialis

occupational hygiene handled, stored and processed. Workers should wash hands and face before eating,
drinking and smoking. Remove contaminated clothing and protective equipment before
entering eating areas. See also Section 8 for additional information on hygiene:
measures.

Conditions for safe storage, : Store in accordance with local regulations. Store in a segregated and approved area

including any Store in a dry, cool and well-ventilated area, away from incompatible materials (see

incompatibilities Section 10). Keep container tightly closed and sealed until ready for use. Cylinders
should be stored upright, with valve protection cap in place, and fimly secured to
prevent falling or being knocked over. Cylinder temperatures should not exceed 52 °C
(125 °F).
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Section 8. Exposure controls/personal protection

Control parameters

0 R -

Ingredient name

Exposure limits

NITROGEN, REFRIGERATED LIQUID Oxygen Depletion [Asphyiant]

Appropriate engineering
controls

Environmental exposure
controls

Individual protection measures
Hygiene measures.

Hand protection

: Good general ventilation should be sufficient to control worker exposure to airbome

contaminants.

+ Emissions from ventilation or work process equipment should be checked to ensure

they comply with the requirements of environmental protection legislation. In some:
cases, fume scrubbers, fiters or engineering modifications to the process equipment

will be necessary to reduce emissions to acceptable levels.

: Wash hands, forearms and face thoroughly after handiing chemical products, before

eating, smoking and using the lavatory and at the end of the working period
Appropriate techniques should be used to remove potentially contaminated clothing
Wash contaminated clothing before reusing. Ensure that eyewash stations and safety
showers are close to the workstation location.

+ Safety eyewear complying with an approved standard should be used when a risk

assessment indicates this is necessary to avoid exposure to liquid splashes, mists,
gases or dusts. If contactis possible, the following protection should be wom, unless
the assessment indicates a higher degree of protection: safety glasses with side-
shields

: Chemical-resistant, impervious gloves complying with an approved standard should be

wom at all times when handiing chemical products if a risk assessment indicates this is
necessary. If contact with the liquid is possible, insulated gloves suitable for low
temperatures should be wom. Considering the parameters specified by the glove
manufacturer, check during use that the gloves are stil retaining their protective
properties. It should be noted that the time to breakthrough for any glove material may
be different for different glove manufacturers. In the case of mixtures, consisting of
several substances the protection time of the gloves cannot be accurately estimated.
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