	
	
	



 

	

MRAD 240 – Specialized Imaging 1
Lab #3 – Activity - Features of C-Arm and Mobile Checklist

Instructions: Check off tasks as completed.

Identify and locate the following features of the C-arm
	
	Feature

	
	Location on C-arm where cable from the monitor plugs in

	
	The connection sequence of cables and power source

	
	On/off switch locations

	
	Exposure switch(es)  

	
	Visual indicators displaying radiation is in use

	
	Brakes and steering handles of monitor and c-arm

	
	Vertical button for height adjustment

	
	Arm extension lock

	
	Wig-wag lock

	
	AP/PA to lateral lock

	
	Horizontal lateral lock










Identify and locate the following features of the Mobile X-ray Machine

	
	Feature

	
	Power on and off

	
	Detector/grid features

	
	Collimator, field size

	
	Tape measure

	
	Technique features

	
	Switch for radiation on/off

	
	Exposure switch

	
	Accessory equipment required

	
	Drive and brake controls

	
	Tube movement/locks

	
	Password protect feature
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